


**High Pressure Simplex Strainers**

**For higher pressure duties we are able to offer a simplex strainer range that can extend the working pressure of the basket strainer up to a maximum of 414 Barg (6000 psi) for a ANSI 2500 rating.   
  
Manufactured in carbon steel or stainless steel and fitted with stainless steel baskets in any perf or mesh size (see**[**simplex web page**](http://www.oxfordfiltration.com/simplexStrainers.asp)**for dimensions), they can be fitted with any flange standard but most frequently ANSI 900, 1500, 2500 and SAE.**



|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **BORE SIZE** | **COMMON DIMENSIONS (mm)** | | | | | **MASS (dry)** |
|  | | | | | | |
|  | A | B | C | D | E | Kg |
| DN20 | 300 | 216 | 200 | 350 | 445 | - |
| DN25 | - |
| DN32/40 | 230 | 400 | 475 | - |
| DN50 | 350 | 240 | 415 | 485 | - |
| DN65 | 240 | 415 | - |
| DN80 | 470 | 268 | 260 | 435 | - |